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1 Introduction, planning
1.1 General Introduction

Objectives of the project

· The objective of the Bull bag version project is to 

· Take over the Expression sales at 99 Euro since it is approaching its end of life time

· To repair the margin at 99 Euro 

(> 10% and > 35% vs. 8% and 32%)

· Extend our Energy Care range to the 99 Euro price point with 1600W

· To extend the supplier base with a new supplier
· The objective of the Bull bagless project is to 

· Introduce a Q2 proposition in WE and Q3 proposition in CEE

· To repair loss in market share in bagless

· To extend the supplier base with a new supplier
· For this project we intend to use an OTS product of an ODM/OEM supplier

1.2 IPD milestones
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Project Plan Committed 

PPC: 
wk 1013
Product Validated 

PV:
wk 1025
Commercial Release 

CR: 
wk 1028
1.3 Introduction Regions/countries, Quantities, Price
	Type
	Total Sales WE
	Total Sales EE
	Total Sales APMEA
	Total sales per type

	FC8130
	221000
	97000
	4000
	322000

	FC8132
	10000
	66000
	15000
	91000

	FC8134
	62000
	38000
	24000
	124000

	FC8136
	199000
	 
	 
	199000

	FC8140
	62000
	6000
	 
	68000

	FC8142
	31000
	 
	4000
	35000

	Total
	585,000 
	207,000 
	47,000 
	839,000 


	FSP Price
	FSP €
	Average IIP
	Average NNP
	Going Price

	FC8130
	€ 28.64 
	€ 37.13 
	€ 49.50 
	€ 99 

	FC8132
	€ 28.64 
	€ 37.13 
	€ 49.50 
	€ 99 

	FC8134
	€ 27.69 
	€ 37.13 
	€ 49.50 
	€ 99 

	FC8136
	€ 27.69 
	€ 37.13 
	€ 49.50 
	€ 99 

	FC8140
	€ 31.13 
	€ 40.88 
	€ 54.50 
	€ 109 

	FC8142
	€ 32.08 
	€ 44.63 
	€ 59.50 
	€ 119 


1.4 Consumer Service Offering (CSO) and repair process
	Region
	CSO

Front end
	CSO

Back end
	Repair process

	WE
	Call center FAQ
Web support FAQ
DFU / User manual

Leaflet
	Repair/ carry in 
	Module swap / scrap 

	EE
	Call center FAQ
Web support FAQ
DFU / User manual

Leaflet
	Repair/ carry in 
	Module swap / scrap 

	APMEA
	Call center FAQ
Web support FAQ
DFU / User manual

Leaflet
	Repair/ carry in 
	Module swap / scrap 


2 Technical specifications

2.1 Range overview
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2.2 Product specifications
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F Specification
items
Bag— FCB134, Bagless — FC8140, | Bag— FCB130,
FCB136 FCB142 FCB132
Motor KingClean KingClean KingClean
IEC1400W IECT800W IEC1800W
Suction Power ‘min 375W at 0-hour | Average = 300W at ‘min 375W at 0-
Average 2350W | 0-hour hour

after 1 year use in
households

meaning 156

Looking at 350W
(depends on the air

Looking at 400W
(depends on the

times cleaning data from EB) air data from EB)
jobs.
(Suction power TBC
measurement after T8C
1 yr life time cyclic
switch test AKS
0604-001)
Suction power <25W <25W <25W
drop during
cleaning job
Dust Loading Not applicable Suction power Not applicable
Performance for decrease <0.6W/g
appliances (dust collection up to
150g) , AKS 000-
0601/038

Vacuum at min
position suction
power knob

Between 80 — 140
mbar

Between 80 — 140
mbar

Between 80 — 140
mbar

Minimum usable

30 lires (Philips S-

7.7 fitres (Dust

3.0 litres (Philips

volume of dust | bag) compartment S-bag)

receptacle 3.2litres (Bull dust | capacity) 32 litres (Bull dust
chamber) chamber)

Air stream Not applicable (Acc. AKS 000- Not applicable

blocking for DMS 0601/014 no

blocking is allowed)

Sound power level | L. < 80dB L. <82dB L. <80dB

for appliances

End user =38 >38 238

satisfaction index

Aesthetics Acc. UN-D-1235 | Acc. UN-D-1235 Acc. UN-D-1235
(tbd) (tbd) (tbd)

Vacuum for 2235kPa tbe tbe

appliance

(measure from the





2.3 New commercial features
· The bag type 1600W product should be awarded by green tick logo with the highly efficient motor (1600W input --> > 375W suction power)
· Products need to comply the sustainability requirements of CL

2.4 Commercial Accessories 
- FC8070 HEPA Outlet filter

- FC8071 Dust container filter set (HEPA + foam)
- Dust bags FC8021, FC8022, FC8023
3 Architecture and characteristics
3.1 Mechanical
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Bagless versions:




Bag versions:
3.2 Electrical

220V China:
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3.3 Critical spare parts

- Motor
- PCB

- Cord winder

- HEPA Exhaust filter
- Dust container filterset
- Hose assy

- Tube assy

- Nozzle(s)

- Cone filter

- S-Bag holder

3.4 Consumer replaceable parts 

- HEPA Exhaust Filter (FC8070)
- Dust container filterset (FC8071)

- Hose assy

- Tube assy

- Nozzle(s)
- Dust container assy

- Cone filter

- S-Bag holder
4 Cost of non quality prediction
4.1 Call center cost
(Cost per call = average time * cost per minute)

	Region
	Amount of calls
	Total Sales
	ACR %
	Average call time
	Price per minute
	Price per call

	WE
	1055
	211K
	0,5
	10min
	€ 1
	€ 10

	APMEA
	165
	33K
	0,5
	7min
	€ 0,20
	€ 1,40


· ACR = Amount of calls / total sales
4.2 CPI (Cost per Intervention)
	NNP
	 WE 
	 EE 
	 APMEA 

	Average retail price (NNP)
	€ 52.00 
	€ 52.00 
	€ 52.00 

	CPI repair
	 
	 
	 

	Additional retail cost's
	€ 4.00 
	€ 1.00 
	€ 1.00 

	Transportation cost's
	€ 10.00 
	€ 7.50 
	€ 0.00 

	Repair labour cost
	€ 11.30 
	€ 10.00 
	€ 2.66 

	Average Discount spares
	30%
	26%
	0%

	Sparepart cost's
	€ 5.62 
	€ 5.95 
	€ 8.04 

	Service concept that will be applied
	Carry in repair
	Carry in repair
	Carry in repair

	CPI exchange
	 
	 
	 

	Retail transportation cost's?
	€ 10.00 
	€ 7.50 
	€ 0.00 

	Retail fee
	€ 5.00 
	€ 5.00 
	€ 2.00 

	Appliance cost's (IIP price)
	€ 39.00 
	€ 39.00 
	€ 39.00 

	Total repair
	€ 30.92 
	€ 24.45 
	€ 11.70 

	Total exchange
	€ 54.00 
	€ 51.50 
	€ 41.00 


4.3 Predicted Field Quality (PFQ) or Field Call Rate (FCR) 

Best estimation at PV is:
FC8134 FC8136: 1.9%
FC8130 FC8132: 2.3%
FC8140 FC8142: 2.3%
4.4 ConQ (Cost of non Quality) 
	 
	CPI repair €
	CPI exch. €
	Exchange vs repair rate
	CPI mix €
	FCR
	Total sales
	CoNQ total

	 WE 
	30.92 
	54.00 
	5%
	€ 32.08 
	2.33%
	  585,000 
	€ 437,247 

	 EE 
	24.45 
	51.50 
	2%
	€ 24.99 
	2.33%
	  207,000 
	€ 120,516 

	 China 
	11.70 
	41.00 
	1%
	€ 11.99 
	2.33%
	    47,000 
	€ 13,129 

	 Total sales 
	 
	 
	 
	 
	 
	839000
	 

	 CPI (avg/weighted) 
	 
	 
	 
	€ 29.20 
	 
	
	 

	Call center cost Europe
	 
	 
	 
	 
	 
	 
	€ 29,250 

	Call center cost APMEA
	 
	 
	 
	 
	 
	 
	€ 329 

	CoNQ (Euro)
	 
	 
	 
	 
	 
	Total CoNQ
	€ 600,141 

	CoNQ (% sales)
	 
	 
	 
	 
	 
	 
	1.38%


4.5 Fast feedback program

	Feedback
	regions
	Quantity 
	cost 

	Rapid exchange Bag version
	WE
	50
	€ 2500

	
	
	Total fast feedback cost
	€ 2500


5 Consumer care package planning

5.1 Consumer care package

	
	 
	Yes/No
	Accountable
	Responsible

	In-box
	 
	 
	 
	 

	 
	User Manual
	Yes
	ARC
	CMM

	 
	Quick Start Guide 
	No
	ARC
	CMM

	 
	Consumer Care Leaflet
	 Yes
	DFU
	CMM

	 
	 
	 
	
	

	Web
	 
	 
	
	

	 
	Leaflet and Photo's
	Yes
	DFU/ARC
	CMM

	 
	FAQ's
	Yes
	ARC
	CMM

	 
	Tips and Tricks
	Yes
	CMM / Marcom
	CMM

	 
	Instruction movies (tutorials)
	no
	Marcom
	CMM

	 
	 
	 
	
	

	Call Center
	 
	 
	
	

	 
	Callcenter Scripts and Tips
	no
	CCQ/ARC
	CMM

	 
	Training package - technical and soft skills
	no
	CCQ/ARC
	CCQ/ARC

	 
	Training execution
	no
	CCQ/ARC
	CCQ/ARC

	 
	Product samples
	Yes
	CMM
	CMM

	 
	 
	 
	
	

	Repair & Exchange
	 
	 
	
	

	 
	Service Manual
	 Yes
	CCQ
	CCQ

	 
	Diagnostics- and Service Tools 
	 no
	CCQ
	CCQ

	 
	Service Bill of Material, incl. spare parts Purchasing Master data
	Yes 
	CCQ
	CCQ

	 
	Training package diagnostics & repair
	 no
	CCQ
	CCQ


5.2 Special phone number

For Europe 800-number will be added to user manual and quick start guide: 

	Country
	# Type
	Consumer 

Phone #
	date

	France
	Free phone
	0805025510
	Live

	Netherlands
	Free phone
	08000230076
	April

	Spain
	Free phone
	900800655
	Live

	UK
	Free phone
	08003316015
	April 15

	Italy
	Free phone
	0800088774
	April 6

	Germany
	Free phone
	08000007520
	Live


5.3 FAQ (Frequently Asked Questions)

FAQ will be translated in to following languages.

- English, French, Danish, Spanish, Italian, Dutch (for all versions)

- Portuguese (additional for Latam version)

- Chinese Simplified (additional for China version)

Attachment 1: Explanation abbreviations  

VPD:
Value Proposition Debriefing

AA:
Assignment Agreed

PPC:
Project Plan Committed

CC:
Concept Consolidation

PC:
Prototype Consolidation

PV:
Product Validated

IR:
Industrial Release

CR:
Commercial Release

PE:
Project end

FSP:
Factory Standard Price 

IIP:
Internal Invoice Price (FSP + NSO costs)

DFU:
Direction For Use

FAQ:
Frequently Ask Questions
PFQ:
Predicted Field Quality
CSO:
Consumer Service Offering

ConQ:
Cost of non Quality

ACR:
Average contact Rate
FCR:
Field Call Rate

FAQ:
Frequently Ask Questions.  

LATAM 
= Latin America

APMEA

= Asian Pacific, Middle East, Africa

Europe

= Europe 
CMM: Elise Michel-Paulsen
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